{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["sheet"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904"}

{"sheet":"sheet","index":0,"n_rows":11,"n_cols":31,"rows_kept":11,"cut":false,"hidden":false,"merged":[[6,5,6,8],[2,0,5,2]]}
[null,null,null,null,"Lat-d° ","Lat-m' ","Long-d°","Long-m' ",null,null,null,null,null,null,null,null,"To start calculations,"]
[null,null,null,null,35,1,135,44,null,null,null,null,null,null,null,null,"option+command+t (Mac)"]
["DO NOT insert/delete any columns and rows in this blue area",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ctrl+t (win)"]
[null,null,null,null,"Reference height of measurement [m]"]
[null,null,null,null,1.1000000000000001]
[null,null,null,null,"Height of anemometer [m]"]
[null,null,null,"Enter RH or WBT or hPa or x",16.2,"Input data by four component radiometer"]
["date","time","ta","RH","vel","Kd","Ku","Ld","Lu","Solar absorptance of cloths","Solar transmittance of cloths","clo","met","representative temperature",null,null,null,null,null,null,"ETU","NUATF","TVF","SERFL","ERFS","SEHF","TVFr","TVFe","EVCF","tsk","w"]
["[ymd]","[h:m:s]","[°C]",null,"[m/s]","[W/m2]","[W/m2]","[W/m2]","[W/m2]","[dimensionless]","[dimensionless]","[clo]","[met]","[°C]",null,null,null,null,null,null,"[°C]","[°C]","[°C]","[°C]","[°C]","[°C]","[°C]","[°C]","[°C]","[°C]","[dimensionless]"]
["2012-07-31","13:00:00",30,60,3,900,133,300,450,0.5,0.1,0.4,2,28.81,"/___","input data",null,null,"results","___\\",31.420986085608064,1.1900005340576172,-2.915521192324952,-8.5764966042589776,12.856242122738983,0.80896464700810311,6.4797617594401045,-7.232964646995196,-3.6687240798800436,34.967747323344568,0.48160816371076803]
["2012-07-31","15:00:00",31,60,2,800,120,300,450,0.5,0.1,0.4,2,28.81,null,null,null,null,null,null,33.583329432349501,2.1900005340576172,-1.8606821885381479,-9.1764966042589773,14.376691493360267,0.40227133451425534,5.9038167317708332,-7.0632713344987312,-3.0201367912660455,35.237610940486128,0.60547322037958606]